DE HAVILLAND DH-88 COMET
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 5,250 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VNO - Max Structural Cruising Speed | 174 MPH
VNE - Never Exceed Speed | 300 MPH
VLE - Maximum Gear Extension Speed | 150 MPH
VS - Stalling Speed | 74 MPH
VY - Best Rate-of-Climb Speed (sea level) | 140 MPH

Maximum Flap Placard Speeds

Flaps degrees | MPH
Full flaps | 120

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.