FORD TRI–MOTOR
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 10,130 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VA - Maneuvering Speed | 107 MPH
VS - Stalling Speed | 58 MPH
VNE - Never Exceed Speed | 145 MPH
VY - Best Rate-of-Climb Speed (sea level) | 72 MPH
VYSE - Single-engine Best Rate-of-Climb Speed | 75 MPH

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

10,130 | 65 MPH

NOTE: For explanations of speeds used on this tab, see "V-speeds"
in the Learning Center Glossary.